(C)Copyright 2003-2005 Marvell(R).
All rights reserved.
==========================================================

SetupYukonWin.txt created 13-Apr-2005

Readme File for SETUPYUKONWIN.exe v8.24.3.3

Supporting: Marvell Yukon Gigabit Ethernet Controller

Operating Systems:
Windows 98 SE, Windows Me, Windows NT 4.0, Windows 2000, 
Windows XP, Windows Server 2003 




This file contains
 1  Overview
 2  Required File
 3  Installation
 4  Silent Installation
    4.1  Driver Installation
    4.2  Driver Removal
    4.3  Driver Repair
    4.4  Further Options
 5  Troubleshooting


==========================================================


1  Overview
===========


The driver installation package contains the Marvell 
NDIS Miniport Driver for the Marvell Yukon Gigabit 
Ethernet Controller. 

This README file explains how to install the driver 
installation package on a machine running one of the 
following operating systems: 

Windows 98 SE, Windows Me, Windows NT 4.0, Windows 2000, 
Windows XP, Windows Server 2003 



2  Required File
================


To install the driver, the following file is required:

    SetupYukonWin.exe



3  Installation
===============


On plug & play Windows versions the adapter is found, 
identified and configured automatically. Cancel all 
operating system attempts to install the driver 
automatically. 

NOTE: To install the driver you have to be logged in as 
      a user with administrative rights.

To install the driver, proceed as follows:

1. Execute the setup file "SetupYukonWin.exe".
2. Follow the instructions displayed during the 
   installation procedure.



4  Silent Installation
======================


NOTE: Silent installation is not supported for 
      Windows NT 4.0. 

In order to install the driver silently the following 
commands should be executed. 

4.1  Driver Installation
------------------------

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log 
REBOOT=ReallySuppress /qn" 


4.2  Driver Removal
-------------------

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log 
REMOVE=ALL REBOOT=ReallySuppress /qn" 


4.3  Driver Repair
------------------

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log 
REINSTALLMODE=vomus REINSTALL=ALL REBOOT=ReallySuppress 
/qn" 

NOTE: On Windows 98 SE and Windows Me it is recommended 
      to use "REBOOT=Force" instead of 
      "REBOOT=ReallySupress" because each driver 
      installation needs a reboot for completion.


4.4  Further Options
--------------------

By default the installation directory is 
"%PROGRAMFILES%\Marvell\Miniport Driver". It can be 
changed by setting the variable "INSTALLDIR". 

Example :

SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log 
INSTALLDIR=C:\MyDir REBOOT=ReallySuppress /qn" 

The installation status is logged in the file 
"%WINDIR%\YukonInstall.log". The log file path and name 
can be changed by replacing "%WINDIR%\YukonInstall.log" 
with the preferred file path and name. 



5  Troubleshooting
==================


If you should encounter any problems with your driver 
installation package, please re-read the instructions 
above and the documentation supplied with the operating 
system carefully. 

Additionally refer to your system event log file (using 
the Event Viewer) and check it for entries from the 
Marvell NDIS Miniport Driver. If your particular problem 
is not listed or the error persists, please send your 
system event log file to our technical support. 

For further information please contact our support.


*** End of Readme File ***


