    ©Copyright 2003-2005 Marvell®.
    All rights reserved.

    SetupYukonWin.htm created 13-Apr-2005

    Readme File for SETUPYUKONWIN.exe v8.24.3.3

    Supporting: Marvell Yukon Gigabit Ethernet Controller

    Operating Systems:
    Windows 98 SE, Windows Me, Windows NT 4.0, Windows 2000,
    Windows XP, Windows Server 2003

# This file contains

1 Overview
2 Required File
3 Installation
4 Silent Installation

4.1 Driver Installation
4.2 Driver Removal
4.3 Driver Repair
4.4 Further Options

5 Troubleshooting

## 1 Overview

    The driver installation package contains the Marvell
    NDIS Miniport Driver for the Marvell Yukon Gigabit
    Ethernet Controller.

    This README file explains how to install the driver
    installation package on a machine running one of the
    following operating systems:

    Windows 98 SE, Windows Me, Windows NT 4.0, Windows 2000,
    Windows XP, Windows Server 2003

## 2 Required File

    To install the driver, the following file is required:

        SetupYukonWin.exe

## 3 Installation

    On plug & play Windows versions the adapter is found,
    identified and configured automatically. Cancel all
    operating system attempts to install the driver
    automatically.

    NOTE: To install the driver you have to be logged in as
          a user with administrative rights.

    To install the driver, proceed as follows:

    1. Execute the setup file "SetupYukonWin.exe".
    2. Follow the instructions displayed during the
       installation procedure.

## 4 Silent Installation

    NOTE: Silent installation is not supported for
          Windows NT 4.0.

    In order to install the driver silently the following
    commands should be executed.

4.1 Driver Installation

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    REBOOT=ReallySuppress /qn"

4.2 Driver Removal

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    REMOVE=ALL REBOOT=ReallySuppress /qn"

4.3 Driver Repair

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    REINSTALLMODE=vomus REINSTALL=ALL REBOOT=ReallySuppress
    /qn"

    NOTE: On Windows 98 SE and Windows Me it is recommended
          to use "REBOOT=Force" instead of
          "REBOOT=ReallySupress" because each driver
          installation needs a reboot for completion.

4.4 Further Options

    By default the installation directory is
    "%PROGRAMFILES%\Marvell\Miniport Driver". It can be
    changed by setting the variable "INSTALLDIR".

    Example :

    SetupYukonWin.exe /S /V"/LIME %WINDIR%\YukonInstall.log
    INSTALLDIR=C:\MyDir REBOOT=ReallySuppress /qn"

    The installation status is logged in the file
    "%WINDIR%\YukonInstall.log". The log file path and name
    can be changed by replacing "%WINDIR%\YukonInstall.log"
    with the preferred file path and name.

## 5 Troubleshooting

    If you should encounter any problems with your driver
    installation package, please re-read the instructions
    above and the documentation supplied with the operating
    system carefully.

    Additionally refer to your system event log file (using
    the Event Viewer) and check it for entries from the
    Marvell NDIS Miniport Driver. If your particular problem
    is not listed or the error persists, please send your
    system event log file to our technical support.

    For further information please contact our support.

    *** End of Readme File ***