Soundscape S-2000 Release Notes

Date: 05/22/95
Version: 1.30.03

--------------------------------------------------------------------------------------------------------------------------------
Troubleshooting Information
--------------------------------------------------------------------------------------------------------------------------------
For up-to-date automated troubleshooting assistance, please call Ensoniq's
Fax-on-Demand service at 1-800-257-1439 from a touch-tone telephone.  
This service requires that you have access to a FAX machine.   Please request
document #7255 (Trouble Shooting Manual).

--------------------------------------------------------------------------------------------------------------------------------
v 1.30.03
--------------------------------------------------------------------------------------------------------------------------------
**SSInit**
SSInit now correctly handles board not detected errors.  The previous version
of SSInit would write out an incorrect value to the SNDSCAPE.INI file if the
Soundscape base address was not detected. 

**Windows Driver**
This version of the driver now correctly restores the Soundscape DOS 
interrupts after a Windows session.  The previous version of the drivers left 
the Soundscape board programmed with the Windows interrupts after exiting 
Windows.  The net result was that DOS games would not run after a Windows 
session unless the Soundscape board was re-initialized.

**SUPER IMPORTANT INFORMATION FOR REVEAL SC600 REV1 OWNERS**
The Windows driver is now backwards compatible with early Soundscape boards
having the TDA8421 tone control chip.  This backwards compatibility is activated
by the assignment IsDvb=Yes in the [sndscape.drv] section of the SYSTEM.INI
file.
