EPSON Imaging Technology Center

Final Release Notes for 
AutoCAD ADI Driver for EPSON ESC/P2 InkJet Printers
version 2.50  
Oct. 9, 1997

Product Description

This driver is a protected mode ADI 4.2 driver for AutoCAD Release 12 and 13 for DOS.  It also runs on release 10 and 11 as well as some additional AutoDESK applications.  
This driver version was developed primarily to support the new EPSON Stylus COLOR 600, 800 and 3000.  The driver also supports all Epson ESC/P 2 monochrome and color inkjet printers released before January 1997.  The code and copyright are owned by Seiko-Epson Corporation.

The following files are included in this release:

 Driver files for AutoCAD 386 (DOS) Release 10-13:

 PLEPSCE.EXP		US English
 PLEPSCU.EXP		UK English
 PLEPSCF.EXP		French
 PLEPSCI.EXP		Italian
 PLEPSCG.EXP		German
 PLEPSCS.EXP		Spanish
 PLEPSCP.EXP		Portuguese
 PLEPSCB.EXP		Brazilian Portuguese

User instruction files (DOS text format):

 READMEUS.TXT		US English
 READMEUK.TXT		UK English
 LISEZMOI.TXT		French
 LEGGIMI.TXT		Italian
 LIESMICH.TXT 		German
 LEAME.TXT			Spanish
 LEIA-ME.TXT		Portuguese

Development files :

Cover.txt			

Installation 

Refer to the localized README text file for instructions on how the driver should be installed.  Follow the "INSTALLING THE DRIVER SOFTWARE" and "CONFIGURING AUTOCAD" sections.

Version Update Description 

This release of version 2.50 contains supports only Ink Jet printers.   This version replaces the Ink Jet printer support found in the previous version 2.40 driver.  The improvements in version 2.50 are as follows:

Provides added support for three new printers: the EPSON Stylus COLOR 600, EPSON Stylus COLOR 800, and EPSON Stylus COLOR 3000.  The 1440x720 resolution feature of Stylus COLOR printers is not supported in this version.

Technical Limitations and Special Notices

1) See Cover.txt file for specific information related to Beta1 review by the ESC’s.

2) A Brazillian Portuguese readme file is not included.  It has never been translated by Epson America, Inc.