$#KINT  xx Search Keys

This compilation of the Interrupt List has only a short version of interrupt search keys. One reason to reduce the number of search keys is that WinHelp v. 4.00 (coming with Windows 95) has a limited keyword capacity.

The following table lists examples of the unavailable long search key format and corresponding short key format:

Instead of the long key:	Use the short key:	
INT 00	00	
INT 02 SI = 0714	02 SI0714	
INT 03 AH = 09	03 09	
INT 03 AX = 0910	03 0910	
INT 10 AX = 007F BH = 00	10 007F BH00	
INT 10 AH = 0B BH = 00	10 0B BH00	
INT 10 AH = 0E CX = ABCD	10 0E CXABCD	
INT 10 AX = 0F56 BX = 4756	10 0F56 BX4756	
INT 88 AL = 00	88 --00	
INT 94 AL = 01 SI = 8017	94 --01 SI8017